Loading data flow

.mff and .raw are two different data formats, which contain the same data files. It should be noted that the electrode file does not need to be replaced when loading .mff, and the electrode file needs to be replaced when loading .raw. The following is the command to load data in EEGlab software.

1. Load the .mff format file:

EEGLAB ->File->Using EEGLAB functions and plugins->From Import Philips .mff file

1. Load the .raw format file:

EEGLAB ->File->Using EEGLAB functions and plugins->From Netstation binary simple file